/* Definitions of prototypes for MIPS built-in functions.  -*- C -*-
   Copyright (C) 2007-2020 Free Software Foundation, Inc.

This file is part of GCC.

GCC is free software; you can redistribute it and/or modify
it under the terms of the GNU General Public License as published by
the Free Software Foundation; either version 3, or (at your option)
any later version.

GCC is distributed in the hope that it will be useful,
but WITHOUT ANY WARRANTY; without even the implied warranty of
MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
GNU General Public License for more details.

You should have received a copy of the GNU General Public License
along with GCC; see the file COPYING3.  If not see
<http://www.gnu.org/licenses/>.  */

/* Invoke DEF_MIPS_FTYPE (NARGS, LIST) for each prototype used by
   MIPS built-in functions, where:

      NARGS is the number of arguments.
      LIST contains the return-type code followed by the codes for each
        argument type.

   Argument- and return-type codes are either modes or one of the following:

      VOID for void_type_node
      INT for integer_type_node
      POINTER for ptr_type_node

   (we don't use PTR because that's a ANSI-compatibillity macro).

   Please keep this list lexicographically sorted by the LIST argument.  */
DEF_MIPS_FTYPE (1, (DF, DF))
DEF_MIPS_FTYPE (2, (DF, DF, DF))
DEF_MIPS_FTYPE (1, (DF, V2DF))

DEF_MIPS_FTYPE (2, (DI, DI, DI))
DEF_MIPS_FTYPE (2, (DI, DI, SI))
DEF_MIPS_FTYPE (3, (DI, DI, SI, SI))
DEF_MIPS_FTYPE (3, (DI, DI, USI, USI))
DEF_MIPS_FTYPE (3, (DI, DI, V2HI, V2HI))
DEF_MIPS_FTYPE (3, (DI, DI, V4QI, V4QI))
DEF_MIPS_FTYPE (2, (DI, POINTER, SI))
DEF_MIPS_FTYPE (2, (DI, SI, SI))
DEF_MIPS_FTYPE (2, (DI, USI, USI))
DEF_MIPS_FTYPE (2, (DI, V2DI, UQI))

DEF_MIPS_FTYPE (2, (INT, DF, DF))
DEF_MIPS_FTYPE (2, (INT, SF, SF))
DEF_MIPS_FTYPE (2, (INT, V2SF, V2SF))
DEF_MIPS_FTYPE (4, (INT, V2SF, V2SF, V2SF, V2SF))

DEF_MIPS_FTYPE (1, (SF, SF))
DEF_MIPS_FTYPE (2, (SF, SF, SF))
DEF_MIPS_FTYPE (1, (SF, V2SF))
DEF_MIPS_FTYPE (1, (SF, V4SF))

DEF_MIPS_FTYPE (2, (SI, DI, SI))
DEF_MIPS_FTYPE (2, (SI, POINTER, SI))
DEF_MIPS_FTYPE (1, (SI, SI))
DEF_MIPS_FTYPE (2, (SI, SI, SI))
DEF_MIPS_FTYPE (3, (SI, SI, SI, SI))
DEF_MIPS_FTYPE (1, (SI, UQI))
DEF_MIPS_FTYPE (1, (SI, UV16QI))
DEF_MIPS_FTYPE (1, (SI, UV2DI))
DEF_MIPS_FTYPE (1, (SI, UV4SI))
DEF_MIPS_FTYPE (1, (SI, UV8HI))
DEF_MIPS_FTYPE (2, (SI, V16QI, UQI))
DEF_MIPS_FTYPE (1, (SI, V2HI))
DEF_MIPS_FTYPE (2, (SI, V2HI, V2HI))
DEF_MIPS_FTYPE (1, (SI, V4QI))
DEF_MIPS_FTYPE (2, (SI, V4QI, V4QI))
DEF_MIPS_FTYPE (2, (SI, V4SI, UQI))
DEF_MIPS_FTYPE (2, (SI, V8HI, UQI))
DEF_MIPS_FTYPE (1, (SI, VOID))

DEF_MIPS_FTYPE (2, (UDI, UDI, UDI))
DEF_MIPS_FTYPE (2, (UDI, UV2SI, UV2SI))
DEF_MIPS_FTYPE (2, (UDI, V2DI, UQI))

DEF_MIPS_FTYPE (2, (USI, V16QI, UQI))
DEF_MIPS_FTYPE (2, (USI, V4SI, UQI))
DEF_MIPS_FTYPE (2, (USI, V8HI, UQI))
DEF_MIPS_FTYPE (1, (USI, VOID))

DEF_MIPS_FTYPE (2, (UV16QI, UV16QI, UQI))
DEF_MIPS_FTYPE (2, (UV16QI, UV16QI, UV16QI))
DEF_MIPS_FTYPE (3, (UV16QI, UV16QI, UV16QI, UQI))
DEF_MIPS_FTYPE (3, (UV16QI, UV16QI, UV16QI, UV16QI))
DEF_MIPS_FTYPE (2, (UV16QI, UV16QI, V16QI))

DEF_MIPS_FTYPE (2, (UV2DI, UV2DI, UQI))
DEF_MIPS_FTYPE (2, (UV2DI, UV2DI, UV2DI))
DEF_MIPS_FTYPE (3, (UV2DI, UV2DI, UV2DI, UQI))
DEF_MIPS_FTYPE (3, (UV2DI, UV2DI, UV2DI, UV2DI))
DEF_MIPS_FTYPE (3, (UV2DI, UV2DI, UV4SI, UV4SI))
DEF_MIPS_FTYPE (2, (UV2DI, UV2DI, V2DI))
DEF_MIPS_FTYPE (2, (UV2DI, UV4SI, UV4SI))
DEF_MIPS_FTYPE (1, (UV2DI, V2DF))

DEF_MIPS_FTYPE (2, (UV2SI, UV2SI, UQI))
DEF_MIPS_FTYPE (2, (UV2SI, UV2SI, UV2SI))

DEF_MIPS_FTYPE (2, (UV4HI, UV4HI, UQI))
DEF_MIPS_FTYPE (2, (UV4HI, UV4HI, USI))
DEF_MIPS_FTYPE (2, (UV4HI, UV4HI, UV4HI))
DEF_MIPS_FTYPE (3, (UV4HI, UV4HI, UV4HI, UQI))
DEF_MIPS_FTYPE (3, (UV4HI, UV4HI, UV4HI, USI))
DEF_MIPS_FTYPE (1, (UV4HI, UV8QI))
DEF_MIPS_FTYPE (2, (UV4HI, UV8QI, UV8QI))

DEF_MIPS_FTYPE (2, (UV4SI, UV4SI, UQI))
DEF_MIPS_FTYPE (2, (UV4SI, UV4SI, UV4SI))
DEF_MIPS_FTYPE (3, (UV4SI, UV4SI, UV4SI, UQI))
DEF_MIPS_FTYPE (3, (UV4SI, UV4SI, UV4SI, UV4SI))
DEF_MIPS_FTYPE (3, (UV4SI, UV4SI, UV8HI, UV8HI))
DEF_MIPS_FTYPE (2, (UV4SI, UV4SI, V4SI))
DEF_MIPS_FTYPE (2, (UV4SI, UV8HI, UV8HI))
DEF_MIPS_FTYPE (1, (UV4SI, V4SF))

DEF_MIPS_FTYPE (2, (UV8HI, UV16QI, UV16QI))
DEF_MIPS_FTYPE (2, (UV8HI, UV8HI, UQI))
DEF_MIPS_FTYPE (3, (UV8HI, UV8HI, UV16QI, UV16QI))
DEF_MIPS_FTYPE (2, (UV8HI, UV8HI, UV8HI))
DEF_MIPS_FTYPE (3, (UV8HI, UV8HI, UV8HI, UQI))
DEF_MIPS_FTYPE (3, (UV8HI, UV8HI, UV8HI, UV8HI))
DEF_MIPS_FTYPE (2, (UV8HI, UV8HI, V8HI))

DEF_MIPS_FTYPE (2, (UV8QI, UV4HI, UV4HI))
DEF_MIPS_FTYPE (1, (UV8QI, UV8QI))
DEF_MIPS_FTYPE (2, (UV8QI, UV8QI, UV8QI))

DEF_MIPS_FTYPE (2, (V16QI, CVPOINTER, SI))
DEF_MIPS_FTYPE (1, (V16QI, HI))
DEF_MIPS_FTYPE (1, (V16QI, SI))
DEF_MIPS_FTYPE (2, (V16QI, UV16QI, UQI))
DEF_MIPS_FTYPE (2, (V16QI, UV16QI, UV16QI))
DEF_MIPS_FTYPE (1, (V16QI, V16QI))
DEF_MIPS_FTYPE (2, (V16QI, V16QI, QI))
DEF_MIPS_FTYPE (2, (V16QI, V16QI, SI))
DEF_MIPS_FTYPE (2, (V16QI, V16QI, UQI))
DEF_MIPS_FTYPE (3, (V16QI, V16QI, UQI, SI))
DEF_MIPS_FTYPE (3, (V16QI, V16QI, UQI, V16QI))
DEF_MIPS_FTYPE (2, (V16QI, V16QI, V16QI))
DEF_MIPS_FTYPE (3, (V16QI, V16QI, V16QI, SI))
DEF_MIPS_FTYPE (3, (V16QI, V16QI, V16QI, UQI))
DEF_MIPS_FTYPE (3, (V16QI, V16QI, V16QI, V16QI))

DEF_MIPS_FTYPE (1, (V2DF, DF))
DEF_MIPS_FTYPE (1, (V2DF, UV2DI))
DEF_MIPS_FTYPE (1, (V2DF, V2DF))
DEF_MIPS_FTYPE (2, (V2DF, V2DF, V2DF))
DEF_MIPS_FTYPE (3, (V2DF, V2DF, V2DF, V2DF))
DEF_MIPS_FTYPE (2, (V2DF, V2DF, V2DI))
DEF_MIPS_FTYPE (1, (V2DF, V2DI))
DEF_MIPS_FTYPE (1, (V2DF, V4SF))
DEF_MIPS_FTYPE (1, (V2DF, V4SI))

DEF_MIPS_FTYPE (2, (V2DI, CVPOINTER, SI))
DEF_MIPS_FTYPE (1, (V2DI, DI))
DEF_MIPS_FTYPE (1, (V2DI, HI))
DEF_MIPS_FTYPE (2, (V2DI, UV2DI, UQI))
DEF_MIPS_FTYPE (2, (V2DI, UV2DI, UV2DI))
DEF_MIPS_FTYPE (2, (V2DI, UV4SI, UV4SI))
DEF_MIPS_FTYPE (1, (V2DI, V2DF))
DEF_MIPS_FTYPE (2, (V2DI, V2DF, V2DF))
DEF_MIPS_FTYPE (1, (V2DI, V2DI))
DEF_MIPS_FTYPE (2, (V2DI, V2DI, QI))
DEF_MIPS_FTYPE (2, (V2DI, V2DI, SI))
DEF_MIPS_FTYPE (2, (V2DI, V2DI, UQI))
DEF_MIPS_FTYPE (3, (V2DI, V2DI, UQI, DI))
DEF_MIPS_FTYPE (3, (V2DI, V2DI, UQI, V2DI))
DEF_MIPS_FTYPE (3, (V2DI, V2DI, UV4SI, UV4SI))
DEF_MIPS_FTYPE (2, (V2DI, V2DI, V2DI))
DEF_MIPS_FTYPE (3, (V2DI, V2DI, V2DI, SI))
DEF_MIPS_FTYPE (3, (V2DI, V2DI, V2DI, UQI))
DEF_MIPS_FTYPE (3, (V2DI, V2DI, V2DI, V2DI))
DEF_MIPS_FTYPE (3, (V2DI, V2DI, V4SI, V4SI))
DEF_MIPS_FTYPE (2, (V2DI, V4SI, V4SI))

DEF_MIPS_FTYPE (1, (V2HI, SI))
DEF_MIPS_FTYPE (2, (V2HI, SI, SI))
DEF_MIPS_FTYPE (3, (V2HI, SI, SI, SI))
DEF_MIPS_FTYPE (1, (V2HI, V2HI))
DEF_MIPS_FTYPE (2, (V2HI, V2HI, SI))
DEF_MIPS_FTYPE (2, (V2HI, V2HI, V2HI))
DEF_MIPS_FTYPE (1, (V2HI, V4QI))
DEF_MIPS_FTYPE (2, (V2HI, V4QI, V2HI))

DEF_MIPS_FTYPE (2, (V2SF, SF, SF))
DEF_MIPS_FTYPE (1, (V2SF, V2SF))
DEF_MIPS_FTYPE (2, (V2SF, V2SF, V2SF))
DEF_MIPS_FTYPE (3, (V2SF, V2SF, V2SF, INT))
DEF_MIPS_FTYPE (4, (V2SF, V2SF, V2SF, V2SF, V2SF))

DEF_MIPS_FTYPE (2, (V2SI, V2SI, UQI))
DEF_MIPS_FTYPE (2, (V2SI, V2SI, V2SI))
DEF_MIPS_FTYPE (2, (V2SI, V4HI, V4HI))

DEF_MIPS_FTYPE (2, (V4HI, V2SI, V2SI))
DEF_MIPS_FTYPE (2, (V4HI, V4HI, UQI))
DEF_MIPS_FTYPE (2, (V4HI, V4HI, USI))
DEF_MIPS_FTYPE (2, (V4HI, V4HI, V4HI))
DEF_MIPS_FTYPE (3, (V4HI, V4HI, V4HI, UQI))
DEF_MIPS_FTYPE (3, (V4HI, V4HI, V4HI, USI))

DEF_MIPS_FTYPE (1, (V4QI, SI))
DEF_MIPS_FTYPE (2, (V4QI, V2HI, V2HI))
DEF_MIPS_FTYPE (1, (V4QI, V4QI))
DEF_MIPS_FTYPE (2, (V4QI, V4QI, SI))
DEF_MIPS_FTYPE (2, (V4QI, V4QI, V4QI))

DEF_MIPS_FTYPE (1, (V4SF, SF))
DEF_MIPS_FTYPE (1, (V4SF, UV4SI))
DEF_MIPS_FTYPE (2, (V4SF, V2DF, V2DF))
DEF_MIPS_FTYPE (1, (V4SF, V4SF))
DEF_MIPS_FTYPE (2, (V4SF, V4SF, V4SF))
DEF_MIPS_FTYPE (3, (V4SF, V4SF, V4SF, V4SF))
DEF_MIPS_FTYPE (2, (V4SF, V4SF, V4SI))
DEF_MIPS_FTYPE (1, (V4SF, V4SI))
DEF_MIPS_FTYPE (1, (V4SF, V8HI))

DEF_MIPS_FTYPE (2, (V4SI, CVPOINTER, SI))
DEF_MIPS_FTYPE (1, (V4SI, HI))
DEF_MIPS_FTYPE (1, (V4SI, SI))
DEF_MIPS_FTYPE (2, (V4SI, UV4SI, UQI))
DEF_MIPS_FTYPE (2, (V4SI, UV4SI, UV4SI))
DEF_MIPS_FTYPE (2, (V4SI, UV8HI, UV8HI))
DEF_MIPS_FTYPE (2, (V4SI, V2DF, V2DF))
DEF_MIPS_FTYPE (1, (V4SI, V4SF))
DEF_MIPS_FTYPE (2, (V4SI, V4SF, V4SF))
DEF_MIPS_FTYPE (1, (V4SI, V4SI))
DEF_MIPS_FTYPE (2, (V4SI, V4SI, QI))
DEF_MIPS_FTYPE (2, (V4SI, V4SI, SI))
DEF_MIPS_FTYPE (2, (V4SI, V4SI, UQI))
DEF_MIPS_FTYPE (3, (V4SI, V4SI, UQI, SI))
DEF_MIPS_FTYPE (3, (V4SI, V4SI, UQI, V4SI))
DEF_MIPS_FTYPE (3, (V4SI, V4SI, UV8HI, UV8HI))
DEF_MIPS_FTYPE (2, (V4SI, V4SI, V4SI))
DEF_MIPS_FTYPE (3, (V4SI, V4SI, V4SI, SI))
DEF_MIPS_FTYPE (3, (V4SI, V4SI, V4SI, UQI))
DEF_MIPS_FTYPE (3, (V4SI, V4SI, V4SI, V4SI))
DEF_MIPS_FTYPE (3, (V4SI, V4SI, V8HI, V8HI))
DEF_MIPS_FTYPE (2, (V4SI, V8HI, V8HI))

DEF_MIPS_FTYPE (2, (V8HI, CVPOINTER, SI))
DEF_MIPS_FTYPE (1, (V8HI, HI))
DEF_MIPS_FTYPE (1, (V8HI, SI))
DEF_MIPS_FTYPE (2, (V8HI, UV16QI, UV16QI))
DEF_MIPS_FTYPE (2, (V8HI, UV8HI, UQI))
DEF_MIPS_FTYPE (2, (V8HI, UV8HI, UV8HI))
DEF_MIPS_FTYPE (2, (V8HI, V16QI, V16QI))
DEF_MIPS_FTYPE (2, (V8HI, V4SF, V4SF))
DEF_MIPS_FTYPE (1, (V8HI, V8HI))
DEF_MIPS_FTYPE (2, (V8HI, V8HI, QI))
DEF_MIPS_FTYPE (2, (V8HI, V8HI, SI))
DEF_MIPS_FTYPE (3, (V8HI, V8HI, SI, UQI))
DEF_MIPS_FTYPE (2, (V8HI, V8HI, UQI))
DEF_MIPS_FTYPE (3, (V8HI, V8HI, UQI, SI))
DEF_MIPS_FTYPE (3, (V8HI, V8HI, UQI, V8HI))
DEF_MIPS_FTYPE (3, (V8HI, V8HI, UV16QI, UV16QI))
DEF_MIPS_FTYPE (3, (V8HI, V8HI, V16QI, V16QI))
DEF_MIPS_FTYPE (2, (V8HI, V8HI, V8HI))
DEF_MIPS_FTYPE (3, (V8HI, V8HI, V8HI, SI))
DEF_MIPS_FTYPE (3, (V8HI, V8HI, V8HI, UQI))
DEF_MIPS_FTYPE (3, (V8HI, V8HI, V8HI, V8HI))

DEF_MIPS_FTYPE (2, (V8QI, V4HI, V4HI))
DEF_MIPS_FTYPE (1, (V8QI, V8QI))
DEF_MIPS_FTYPE (2, (V8QI, V8QI, V8QI))

DEF_MIPS_FTYPE (2, (VOID, SI, CVPOINTER))
DEF_MIPS_FTYPE (2, (VOID, SI, SI))
DEF_MIPS_FTYPE (2, (VOID, UQI, SI))
DEF_MIPS_FTYPE (1, (VOID, USI))
DEF_MIPS_FTYPE (3, (VOID, V16QI, CVPOINTER, SI))
DEF_MIPS_FTYPE (3, (VOID, V2DF, POINTER, SI))
DEF_MIPS_FTYPE (3, (VOID, V2DI, CVPOINTER, SI))
DEF_MIPS_FTYPE (2, (VOID, V2HI, V2HI))
DEF_MIPS_FTYPE (2, (VOID, V4QI, V4QI))
DEF_MIPS_FTYPE (3, (VOID, V4SF, POINTER, SI))
DEF_MIPS_FTYPE (3, (VOID, V4SI, CVPOINTER, SI))
DEF_MIPS_FTYPE (3, (VOID, V8HI, CVPOINTER, SI))
